**Water Analysis**

**Applicants must arrange for their water supply to be sampled and tested in Accordance with European Union (Drinking Water) Regulations 2014.**

**Test must be carried out by an Independent Water Quality Laboratory which is accredited to ISO 17025 for testing all parameters listed below. Water Samples must be taken on site by qualified personnel.**

**To qualify for final approval you must arrange second test for the parameters which failed in first test. If results are compliant they must be submitted with paid invoices for completed work.**

**Coliform Bacteria**

**E.coli**

**Arsenic**

**pH**

**Iron**

**Manganese**

**Nitrate**

**Clostridium Perfringens**

**Colour**

**Conductivity @ 20C**

**Fluoride**

**Turbidity**

**Ammonium (NH4)**

**Arsenic**

**Hardness**

**Odour**

**Taste**

**Below Non-Exhaustive list of ISO 17025 Accredited Laboratories.**

**HSE............................. 0494373414**

**City Analysts....................... 016136003**

**Fitz Scientific: ...................... 041 9845440 ext 1**

**Applicants may use labs not listed but they must be fully Accredited.**

**Fully Accredited Labs wishing to add their name to this list should contact Cavan County Council Water Services.**